

OBSOLETE: Sending to different I2C addresses (0x28 and 0x2f)






OBSOLETE: RESULT\_TEST\_I2CtoSPI\_BRIDGE\_ADDRESS 8/3/15

TEST\_I2CtoSPI\_BRIDGE\_ADDRESS

SlotCard 851 – PASSED



SlotCard 918 – NOT PASSED

