TC\_F\_MONITORING\_AGC\_FUNCTIONS

Correctly connected via I2C

